**(LETTERHEAD)**

**CERTIFICATE OF COMPLIANCE OF VEHICLE SWEPT PATH PERFORMANCE**

**GIVING A CATEGORY 2 OVERDIMENSION VEHICLE THE RIGHT TO OPERATE IN ACCORDANCE WITH CATEGORY 1 OVERDIMENSION OPERATING REQUIREMENTS**

**Background**

Land Transport Rule Vehicle Dimension and Mass 2002 (the Rule) specifies requirements for dimension and mass limits for vehicles operating on New Zealand roads. The Rule sets in place a regulatory regime so that vehicles are operated safely.

The Rule includes requirements for overdimension vehicles, including signs, markings and travel restrictions, for overdimension vehicles as ways to manage the risk to public safety. The Rule also recognises that the ability of a vehicle to perform cornering manoeuvres is dependent on factors other than size alone.

Therefore, the Rule provides facility for the road space requirements (swept path) of overdimension vehicles to be assessed so that vehicles of similar performance, and risk to safety, can operate under the same requirements.

**Certification**

Pursuant to section 6.6(12) of the Land Transport Rule Vehicle Dimensions and Mass 2002 Rule 41001 (the Rule) and by way of an appointment from the New Zealand Transport Agency dated the … day of (Month) (Year), I (Certifier), of (Company), verifies the following vehicle meets the specifications of Schedule 9 of the Rule. Therefore, subject to the conditions below the vehicle is granted exemption from complying with the requirements for Category 2 overdimension vehicles and instead, the operating requirements for Category 1 overdimension vehicles as prescribed in the Rule will apply.

**Conditions:**

1. This Certificate shall be rendered void and of no effect if there are any changes to the vehicle that would result in it failing to meet the requirements of Schedule 9 of the Rule or if the attached vehicle specifications are not complied with.
2. This Certificate shall be carried inside the cab of the vehicle at all times and shall upon request be presented to a Police Officer.
3. The operator of this vehicle must comply with all other Acts, regulations and laws pertaining to this vehicle.
4. This Certificate is revocable and shall forthwith be returned to the Director of the NZ Transport Agency on receipt of written notification to that effect from the Director.

Registration Number(s) of vehicle certified: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Certificate Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Vehicle specifications:**

Number of Axles: Vehicle One:\_\_\_\_\_\_\_\_\_ Vehicle Two: \_\_\_\_\_\_\_\_\_\_\_\_

Tyre sizes: Vehicle One: \_\_\_\_\_\_\_\_\_ Front: \_\_\_\_\_\_\_\_\_ Rear: \_\_\_\_\_\_\_\_\_

 Vehicle Two: \_\_\_\_\_\_\_\_\_ Front: \_\_\_\_\_\_\_\_\_ Rear: \_\_\_\_\_\_\_\_\_

*and any other relevant information to effecting vehicle’s ability to comply with Schedule 9 of the rule*

* *include dimensioned drawing of vehicle(s)*

Vehicle sketch with dimensions

Vehicle Specifications

Truck 🞏; Truck/trailer 🞏; Tractor/semi trailer 🞏; Grader 🞏; Truck Crane 🞏;

Trailing Boom Crane 🞏; Other 🞏;

Number of axles and configuration; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Location of steering axles; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Tyre sizes; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Additional conditions affecting compliance with Schedule 8/ Schedule 9 of the Rule;

Special operating conditions;

Inspected by: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ID Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

***Print on the obverse of the Certificate of Compliance for Swept Path Performance (Cat 2)***